	GREEN CHANNEL


HYDERABAD METROPOLITAN DEVELOPMENT AUTHORITY
APPLICATION CUM SCRUTINY FORM FOR LAYOUT APPROVAL
(U/S 18, 19 & 20 of the HMDA ACT, 2008)
								
To
The Metropolitan Commissioner,		
Hyderabad Metropolitan Development Authority,
Tarnaka, Hyderabad – 500 007

	PART   ::  A ::
To be filled  and certified by Architect






Sir / Madam,							  Date: dd.mm.yyyy
	I / We________________________________ s/o __________________________ hereby submit the application cum scrutiny form for approval of Layout to carryout development i.e., plotted layout development in the Site as per the details given below in accordance with Section 18, 19 & 20 of the Hyderabad Metropolitan Development Authority Act, 2008. The necessary enclosures pertaining to the ownership of the site and layout plans drawn to the scale etc. are submitted herewith. We are aware of the guidelines of the Green Channel and abide by the said provisions and request the HMDA to approve under Green Channel.
[1.Use CAPITAL LETTERS only 2. Fill in relevant information 3. Incomplete application will be rejected]

	I
	DETAILS OF APPLICANT[for correspondence]

	1. 
	Name in full
	

	1. 
	Whether the Applicant is Land Owner / Developer 
(Tick the applicable one)
	Land Owner
	

	1. 
	
	Developer
	

	1. 
	If the Applicant is Developer whether the copy of the Agreement of Land Owner and Developer is enclosed
	YES
	

	1. 
	
	NO
	

	1. 
	
	NOT APPLICABLE
	

	1. 
	S/o / W/o
	

	1. 
	Door No./Flat No.
	

	1. 
	Road/Street
	

	1. 
	Village 
	Mandal
	
	

	1. 
	City/ Town
	
	PIN
	
	
	
	
	
	

	1. 
	District
	

	1. 
	Phone / Mobile No.
	

	1. 
	e-mail
	

	II
	DETAILS OF DEVELOPER / DOCUMENT AUDITOR / LICENCED ARCHITECT

	Sl. No.
	Name
	License No.
	Address with mobile No. & email 
	Signature

	1 
	

Land Owner
	
	
	

	2 
	


Developer
	
	
	

	3 
	


Document Auditor 
	
	
	

	4 
	





Licensed Architect
	
	
	

	
	
	
	
	

	III
	DETAILS OF THE LAND PROPOSED FOR LAYOUT APPROVAL

	1 
	Site Area
	
…………..………..Hectares [………Acs……….guntas]


	2 
	
	

…………………….Sq. M  […………………….sq.yds]


	3 
	Survey Nos.
	
	
	
	

	4 
	Village 
	
	
	
	

	5 
	Mandal
	
	
	
	

	6 
	District
	
	
	
	

	7 
	Zone
	
	
	
	

	8 
	Locality /
Nearest Land Mark
	

	9 
	Details of Permission (if any) sanctioned earlier for the site u/r and status on ground
	

	10 
	Details of Permission (if any) sanctioned earlier neighboring to the site and status on ground
	


	IV
	CLASSIFICATION OF LAYOUT:

	1
	Type of layout proposed
[tick the appropriate one]

	
Open Layout 

	

	
	
	
Gated Layout                (with compound wall)

	

	2
	Whether peripheral road provided in case of Gated Layout with compound wall.
The Peripheral Road is mandatory in case the lands in the vicinity and rear side are not having independent access. If the peripheral road is not provided, justification for not providing the peripheral road shall be furnished duly showing the topographical plan to that extent.

Please show the detailed Plan showing the existing and Master plan roads in the site and in the vicinity duly marking the alignment of the peripheral road.
	



	V
	MASTER PLAN DETAILS:
LAND USE & ZONING REGULATION INFORMATION:

	1
	Site u/r falls in the Notified Master Plan [tick the applicable one]

	CDA area
	

	
	
	Erstwhile HUDA area
	

	
	
	HADA
	

	
	
	MDP-2031
	

	
	
	ORR Growth Corridor
	

	2
	Land use as per Notified Master Plan
	


	3
	Land use of the Proposed Layout
	

	4
	Whether proposed activity is permissible as per Zoning Regulations

	YES
	NO

	5
	Whether any Master Plan roads are passing through or abutting to the site
	YES
	NO

	6
	If yes, the width of the existing roads and the roads proposed in Master Plan shall be mentioned duly showing the alignment of them in the Layout Plan.
	YES
	NO

	7
	Whether the Master Plan roads have been incorporated in the layout proposals
	YES
	NO

	8
	Whether the Undertaking is given to handover the Master Pan roads free of cost to the HMDA/Local Body
	YES
	NO

	9

	The extent of the area affected in the Master Plan Roads (in sq. m)
	



	10
	Whether the site is affected by / close to any restricted area:
(tick the applicable one)

	
	a
	Water Bodies
	

	
	b
	Railways
	

	
	c
	Electrical Lines
	

	
	d
	Airport  
	

	
	e
	Defense Establishments
	

	
	f
	Oil / Gas Pipelines
	

	
	g
	Heritage Structures
	

	
	h
	Environmental Clearance
	

	
	i
	ORR Buffer Zone
	

	a
	Water Bodies:
Unless and otherwise stated, the area and the Full Tank Level (FTL) of a Lake / Kunta shall be reckoned as measured and as certified by the Irrigation Department and Revenue Department. Hence the FTL and the actual extent of the water body shall be marked on the ground with the help of Revenue and Irrigation departments and the same shall be shown in the Layout plan.
i. Unless and otherwise stated, the area and the Full Tank Level (FTL) of a Lake / Kunta shall be reckoned as measured and as certified by the Irrigation Department and Revenue Department. 
ii. The above water bodies and courses shall be maintained as Recreational/Green Buffer Zone and no building activity shall be carried out within:
1. 100m from the boundary of the River outside the Municipal Corporation / Municipality / Nagara Panchayat limits and 50m with in the Municipal Corporation / Municipality / Nagara Panchayat limits. The boundary of the river shall be as fixed and certified by the Irrigation Department and Revenue Department.
2. 30m from the FTL boundary of Lakes / Tanks / Kuntas of area 10Ha and above.
3. 9m from the FTL boundary of Lakes / Tanks / Kuntas of area less than 10Ha / shikam lands;
4. 9m from the defined boundary of Canal, Vagu, Nala, Storm Water Drain of width more than 10m.
5. 2m from the defined boundary of Canal, Vagu, Nala, Storm Water Drain  of width up to  10m.

(iii) Unless and otherwise specified in the Master Plan / Zonal Development Plan.
(1) In case of (ii) (1) & (2) above, the buffer zone may be utilised for road of minimum 12m width, wherever feasible.
(2) In case of (ii) (2) above, in addition to development of recreational / green belt along the foreshores, a ring road or promenade of minimum 12m may be developed, wherever feasible.
(3) The above buffer zone to be left may be reckoned as part of tot lot or organized open space and not for setback requirements.
(iv) In case of Protection of Catchment area of Osmansagar and Himayatsagar lakes covered under the G.O.Ms.No.111 MA dated 08.03.1996, the restrictions on building and development activity imposed there in shall be applicable in Hyderabad Metropolitan Development Authority (HMDA) area.
	Nature of Water Body: 
(tick the applicable one)



	River 
	

	
	
	
	Tank
	

	
	
	
	Lake
	

	
	
	
	Kunta
	

	
	
	
	Canal
	

	
	
	
	Vagu
	

	
	
	
	Nala
	

	
	
	
	Storm water drain
	

	
	
	Buffer Zone to be left       as per Rule (in m)
	

	
	
	Buffer Zone left in the Layout Plan    (in m)
	

	
	
	Whether the Layout plans are satisfying the rules as required for Water Bodies?
	
YES

	NO

	
	
	Whether the NOC from the department of Revenue not below the rank of Joint Collector has been obtained? 
	
YES

	NO

	
	
	Whether the NOC from the Irrigation Department not below the rank of Executive Engineer has been obtained?
	
YES

	
NO

	b
	Railways
The distance between the Railway Property Boundary and the edge of the building shall be 30m as per Indian Railways Works Manual or as per No Objection Certificate (NOC) given by the Railway Authorities. { Buffer zone may be proposed for the  distance to be maintained }

	Whether the site is abutting to railway property?
	
YES

	NO

	
	
	If Yes, whether the required 30m buffer zone has been left in the layout plan?
	
YES

	NO

	
	
	If No, whether any NOC from Railway Authorities has been obtained?
	
YES

	NO

	
	
	If Yes, the distance between the Railway Property Boundary and the boundary of the Plot as per NOC. (in m)
	

	
	
	If Yes, the distance between the Railway Property Boundary and the boundary of the Plot shown in the Layout Plan.
(in m)
	

	
	
	Whether the distance (buffer zone for railway property) shown in the proposed Layout Plan is satisfying the rule?
	
YES

	NO

	c
	Electrical Lines
(i) In case of HT Electricity Tower lines, the land all along below the tower line shall be developed as green belt to an extent of the width of tower base and on either side of green belt there shall be a minimum of 10m wide roads or as defined in the Master Plan. 

	Whether there is any HT Electric Tower Lines passing through the site.
	
YES

	NO

	
	
	If Yes, whether the required land all along below the tower line is proposed as green belt to an extent of the width of tower base and on either side of green belt a minimum of 10m wide roads or as defined in the Master Plan is shown in the Proposed Layout Plan? 
If so, give the detailed report.


	
	(ii) In case of the other Electric Lines if passing through the site whether it is proposed to relay them all along the proposed layout roads or to be retained as existing on ground.

	Whether there are any other Electricity lines passing through the site? 
	
YES

	NO

	
	(iii) 
	If yes, in case the same are required to be realigned all along the proposed layout roads, whether any undertaking is submitted to this extent?
	
YES

	NO

	d
	Airport  
Building Restrictions
(1) For building activity within the Restricted Zone / Air Funnel Zone near the airport, necessary clearance from the concerned Airport Authority shall be obtained.
(2) The building heights and other parameters shall be regulated as per the stipulations of the Airport Authority of India as notified in Gazette of India  Extraordinary (S.O.1589) dated 30-06-2008 and as amended from time to time by Ministry of Civil Aviation, Government of India.
(3) Irrespective of their distance from the aerodrome, even beyond 22km limit from the Aerodrome Reference Point, no radio masts or similar installation exceeding 152m in height shall be erected except with the prior clearance from Civil Aviation Authorities.
(4) In respect of any land located within 1000m from the boundary of Military Airport no building is allowed except with prior clearance from the concerned airport authority with regard to building height permissible and safe distance to be maintained between the building and boundary of the aerodrome.
	Whether the site is abutting or in the vicinity of Airport?
	
YES

	NO

	
	
	If yes, whether it is a Civil airport or Military Airport?

	Civil Airport
	Military Airport

	
	
	If so, whether the NOC from the concerned Authorities have been obtained and submitted?
	
YES

	NO

	
	
	Give the details of the orders issued by the authorities.

…………………………………


	e
	Defense Establishments
In case of Sites within 500m distance from the boundary of Defense Areas / Military Establishments prior clearance of Defense Authority shall be obtained.

	Whether the site is abutting to the              defense establishments within a distance of 500m from the site.

	
YES

	NO

	
	
	If yes, the distance from the boundary of Defense Areas / Military Establishments to the boundary of the site.
(in m) [This shall be marked on the layout plan]
	


	
	
	The details of the NOC issued by the            Defense Authority may be given below:

…………………………………




	f
	Oil / Gas Pipelines
In case of Sites in the vicinity of Oil / Gas pipelines, clearance distance and other stipulations of the Respective Authority shall be complied with. 
	Whether the site is in the vicinity of Oil/ Gas pipelines?
	
YES

	NO

	
	
	If yes, whether the NOC from the concerned Authority has been obtained?

	
YES

	NO

	
	
	If Yes, give the details of the conditions given in the NOC. And also show the same on the proposed Layout Plan.

…………………………………

	
	
	Specific Remarks if any.

	g
	Heritage Structures
(i) In case of Sites located within the distance up to 100m from protected monuments as notified under Archeological Monuments and Ancient Sites and Remains Act 1955 and as amended no construction is allowed.
(ii)  For the Sites located within distance of above 100m and up to 200m from the protected monuments, the construction is allowed only after obtaining prior permission from the National Monument Authority.
(iii) For the Sites located within the vicinity of any Heritage Structure notified as per the respective law, the prior clearance from the concerned authority shall be obtained.
(iv) For the development / redevelopment of any notified Heritage Structure the stipulations as prescribed by the respective authority shall be followed.
	Whether the site is located in the vicinity of any heritage structure?
	
YES

	NO

	
	
	If yes, any NOC is obtained from the concerned authority? 
	
YES

	NO

	
	
	And the details of the NOC and to state whether the conditions are followed in the proposed Layout Plan.


…………………………………

	
	
	Specific Remarks if any.

 …………………………………

	h
	Environmental Clearance
If the site area is 50Hectares and above, the Prior clearance from the State Environmental Impact Assessment Authority (SEIAA) is required.

	Site Area

	
……………… Hectares

	
	
	
	
………………sq. m

	
	
	If the site area is 50hecatres and above whether the prior clearance from the State Environmental Impact Assessment Authority (SEIAA) is obtained?
	
YES

	NO
	NOT APPLICABLE

	
	
	If yes, give the details of the conditions and to state whether the same has been shown in the Proposed Layout Plan.

…………………………………


	
	
	Specific Remarks, if any.




…………………………………

	i
	ORR Buffer Zone
All properties abutting ORR mandatorily will have an open Buffer of 15m from the ROW outer edge. 
Access will not be allowed on to the service roads of the ORR directly.
	Open Buffer of 15m from the ROW outer edge is provided
	YES

	NO

	11
	Any other important features close to the site


	

	12
	Whether the Proposed Layout Plan is prepared keeping all the details pertaining to the mandatory restrictions. Give details.
	










	
VI
	
SITE INSPECTION REPORT 
	

	1
	Site inspected by 
(name of the Empanelled Architect)
	

	2
	a. Whether the site is getting access from a minimum 9m wide public road as Approach road?
b. In case ORRGC minimum width of the access road shall be 12m.
	YES
	NO

	
	c. Whether Photograph showing the approach road is enclosed?
	YES
	NO

	3
	Type of approach road 

	Established
	Kucha

	4
	Give the detailed remarks regarding access and approach road to the site
	



	5
	Physical Features within the site:
(tick the appropriate one)
	(All the existing Physical Features within the site shall also be shown       in the Proposed Layout Plan)

	a
	i. Give the detailed remarks on the existing water   bodies in the site and in the vicinity.                       (The natural course of these water bodies shall not be disturbed in the proposed development. Hence the proposed Layout plan shall incorporate these existing developments as per the ground position)
	

	
	ii. Whether the buffer zone is provided for the water bodies as per rules & natural water bodies are preserved?

	YES
	NO

	
	iii. 
	Give details:

	b
	Electrical lines 
(The existing electricity lines may be realigned with the prior permission of the concerned authorities, for which a separate permission is required from them. Before issuing the final layout the approval of the concerned authorities shall be submitted)
	Whether there is any HT Electric Tower Lines passing through the site.
	
YES

	NO

	
	
	If Yes, whether the required land all along below the tower line is proposed as green belt to an extent of the width of tower base and on either side of green belt a minimum of 10m wide roads or as defined in the Master Plan is shown in the Proposed Layout Plan? If so, give the detailed report.
……………………………………………




	
	
	Whether there is any other Electricity lines passing through the site? 
	
YES

	NO

	
	
	If yes, in case the same are required to be realigned all along the proposed layout roads, whether any undertaking is submitted to this extent?
	
YES

	NO

	c
	Water supply lines
i. What is the source of water supply?
	

	
	ii. If the ground water is proposed as a source of water supply, whether the report from the competent authorities has been obtained?
	

	
	iii. Whether any existing pipe lines are available for supplying water? If so give details.

	

	d
	Oil / Gas Pipelines 
(The existing alignment of them shall be marked and the prior NOC from the concerned authorities shall be obtained and the conditions as stipulated by the said authorities shall be followed and the Layout plan also show the alignment and the buffer as stipulated by the authorities)
	

	e
	Roads 
Details existing and proposed roads in the Master plan and Layout plans may be explained.
	

	f
	Other physical features if any



	

	6
	Surrounding developments:
If any layout is developed adjacent to the site, the same shall be furnished duly stating the details of approval given by HMDA / DTCP / Gram panchayat etc., & to enclose a copy of the layout plan. This shall also be incorporated in the topo plan.
	North:

South:

East :

West:


	7
	Other information if any

	
	




	VII
	TECHNICAL REMARKS :

	S. No.
	Description
	As per Rule
	As per Plan
	Remarks

	1
	Site Area
	Min. 4.0 Hectors  (40000sq.m)
	
	

	2
	Approach Road width 



	Minimum 9m

Minimum 12m   (in case of ORRGC areas)
	
	

	3
	Internal Road widths in the proposed Layout
[Residential]

*[in case of ORRGC the minimum width of all internal road shall be 12m for plots other than EWS & LIG]
	Road length as per Rule 
	Width of the Road
	Road length as per Plan
	Width  of the Road as per Plan
	Other Requirements

	
	
	*Up to 300m

	9m
	
	
	Utilities and services to be underground and located preferably under the footpaths and not under the main carriage way

	
	
	Above 300m and up to 500m
	12m
	
	
	

	
	
	Above 500m and less than 1000m

	18m
	
	
	Utilities and services to be underground and located preferably under the footpaths and not under the main carriage way.

Mountable divider essential

	
	
	1000m and above
	36m
	
	
	Utilities and services to be underground and located preferably under the footpaths and not under the main carriage way.

Median and service road development essential.

	4
	Open space [Parks, Play grounds] & Social  infrastructure area to be provided 
(To be handed over to Local Body through registered Gift Deed)
	
	

	
	a. Site area for Parks, Play grounds etc.
(This area shall be compact and shall be preferably in the center of the layout area or in the center of a block of plots, which means that the park area is useful for the entire colony )
	10%                    (in case the site falls in………….)
	


………………%
	

	
	b. 
	7.5%
(in case the site falls in………..)
	………………%
	

	
	c. 
	…………….sq. m
	…………….sq. m
	

	
	d. Social     infrastructure
	2.5% (in case of 


	
………………%

	

	
	e. 
	…………….sq. m
	…………….sq. m
	

	5
	Provision for services for 
Septic Tank / STP, Sump, OHT & Electrical transformer etc.
	To be provided over and above the 10% of the open space area
	………………%


…………….sq. m
	

	6
	Provision of EWS/LIG (This shall be marked on the proposed Layout Plan also)
	a) Providing within the site
	
	

	
	
	i. EWS – 5% 
	
	

	
	
	ii. LIG – 5%
	
	

	
	
	b) Providing outside the site within 5km radius
	
	

	7
	Area to be handed over to HADA free of cost for Capitalization towards Master Plan facilities. 

	a) 5% of the developable area (or)
	
	

	
	
	b) To pay 1.5 times the basic value per sq. yd of such land to HMDA in lieu of such land to be given to HMDA.                     (In case the applicant is willing to pay the amount, he shall pay the same along with the application duly enclosing the latest Basic Value statement obtained from the Registration Department)
	
	

	8
	Area to be mortgaged in favour of HMDA
(The area to be mortgaged shall be demarcated on the proposed Layout Plan and the draft mortgage document shall also be submitted along with the application. 
The area of mortgage shall be the plots abutting to main roads and shall be a contiguous area)
	15% of the saleable area
	
	



	VIII
	LAND USE ANALYSIS OF THE PROPOSED LAYOUT:

	S.
No.
	Particulars
	Area 
in Sq. m
	Percentage to total land
	Remarks

	1
	Plotted area (Regular)
	
	
	

	2
	Plotted area EWS
	
	
	

	3
	Plotted area LIG
	
	
	

	4
	Area earmarked for Amenities
	
	
	

	5
	Area under roads
	
	
	

	6
	a) Site area for Parks, Play grounds etc
	
	
	

	
	b) Area proposed for Social infrastructure
	
	
	

	7
	Utilities area
(Septic tank / STP, OHT, Electrical installations etc.)
	
	
	

	8
	Other purposes
	
	
	

	
	Total
	
	
	



	IX
	PAYMENT OF FEES & CHARGES: 

	A
	Layout Processing Fee:

	S.
No
	Description
	Extent of the land 
(in sq. m)
	Unit Rate
(Rs.)
	Total
(Rs.)
	Amount Paid
(Rs.)
	Balance
(Rs.)

	1

	Layout Processing fee
( @  Rs.10 per Sq. m on total extent)
	
	10.00
	
	
	

	2
	Rupees....

	
	Challan No.
	
	
	
	
	
	
	
	Date
	dd
	mm
	yyyy

	B
	Fee & Charges including Development Charges:

	S.
No
	Description
	Extent of the land 
(in sq. m)
	Unit Rate
(Rs.)
	Total
(Rs.)
	Amount Paid
(Rs.)
	Balance
(Rs.)

	1
	Development Charges on total extent.
(As per G.O. Ms. No. 439 MA  dt. 13-06-2007 & G.O. Ms. No. 275 MA dt. 12-07-2012 in case of extended area)
	
	
	
	
	

	2
	1.5 times to the basic value of 5% of developable land to be handed over to HMDA for Capitalization towards provision of Master Plan facilities 
(as per G.O. Ms. No. 526, 527, 528 dt. 31-07-2008 &G.O. Ms. No. 33 MA dt. 24-01-2013. 
	
	
	
	
	

	3
	External Betterment charges in case of HADA area ( G.O. Ms. No. 287 MA dt. 03-04-2008)
	
	
	
	
	

	4
	Publication Charges (inclusive of postage charges) 
	 
	5,000.00
	5,000.00
	
	

	5
	Others
	
	
	
	
	

	6
	Total
	
	
	
	
	

	7
	Rupees……..

	
	DD No.
(crossed)
	
	
	
	
	
	
	
	Date
	dd
	mm
	yyyy

	
	Bank Name        
	

	
	Branch
	


	X
	C E R T I F I C A T E  B Y  A R C H I T E C T

	
This is to certify that the site situated in Sy. Nos. __________________________ of  ________________ (V) ____________________ (M), ________________District proposed for development has been personally inspected by me and found that the location, measurements, boundaries, extent, width of  approach road and abutting road etc., are in accordance  with plans furnished to HMDA.  It is further certified that the proposals are scrutinized with reference to Master Plan proposals, relevant Government orders, Rules issued from time to time and proposals conform to rules as mentioned in detail in the checklist. The proposals are also scrutinized with reference to Restrictions of building activity in the vicinity of areas such as water bodies, railway properties, electric lines, airport, oil / gas pipe lines, heritage structures, religious structures etc and are found in order.   
The information furnished in the check list is true to the best of my knowledge. I am aware that I am liable for action in the event of non-conformity of any parameter to Master Plan proposals and provisions of relevant Government orders / rules issued from time to time.  

	1
	Name of the 
Architect

	

	
	Address 
	

	
	License No. issued by HMDA:
	

	
	Phone:
	

	
	Signature of the 
Architect
	

	2
	Name of the 
Land  Owner

	

	
	Address 




	

	
	Phone:
	

	
	Signature of the 
Land Owner
	

	3
	Name of the Developer 
	

	
	Address 

	

	
	License No. issued by HMDA:
	

	
	Phone:

	

	
	Signature of the 
Developer
	



	XI
	MANDATORY ENCLOSURES 
To be submitted along with the Application cum Scrutiny Form for Layout Approval)

	Sl. No.
	DOCUMENT DETAILS
	Required/Not required
	Submitted
	Not submitted

	1
	Application for Layout Approval signed by the Owner, Developer, Document Auditor, Architect. 
	
	
	

	2
	Ownership Documents 

	
	
	

	3
	Pattadar Pass Book

	
	
	

	4
	Title Deed issued by Revenue Authority         (Attested by Gazetted Officer)
	
	
	

	5
	Link Documents (Attested by Gazetted Officer)

	
	
	

	6
	Pahanies issued by the Revenue Authority

	
	
	

	7
	Latest Encumbrance Certificate issued by Registration Department
	
	
	

	8
	Development Agreement of Sale cum General Power of Attorney
	
	
	

	9
	Land use Certificate issued by HMDA 

	
	
	

	10
	Licence copy of Architect renewed by COA 
(Attested by Gazetted Officer)

	
	
	

	11
	Licence copy of the Builder / Developer issued by ULB / HMDA
(Attested by Gazetted Officer)
	
	
	

	14
	Certificate by the Empanelled Architect

	
	
	

	15
	Certificate by the Land Owner & Developer

	
	
	

	16
	Latest Land Value Certificate issued by the Registration Department
	
	
	

	17
	Payment of Layout Processing Fee
	
	
	

	
	
Rupees.........      
	
	
	

	
	ChallanNo.
	
	
	
	
	
	
	
	Dt
	dd
	mm
	2014
	
	
	

	18
	Payment of Fee & Development Charges.
	
	
	

	
	
Rupees.........              
	
	
	

	
	DD No.
	
	
	
	
	
	
	
	Date
	dd
	mm
	2014
	
	
	

	
	Bank Name:         

	
	
	

	
	Branch:

	
	
	

	
19
	Draft Mortgage Deed duly indicating the plots proposed for mortgage.
	
	
	

	20
	Draft Gift deed copy for handing over the 5% of the Developable land to HMDA
	
	
	


	
PLANS

	1
	Location Plan (scale 1:1000) of the site and surrounding developments / lands showing surrounding roads, electricity lines of HTL/LTL, Existing Drainage, Sewerage etc. within 500m radius of the site.
	
	
	

	2
	Satellite Imagery for the site and the surrounding developments within 500m radius of the site.

	
	
	

	3
	Detailed Topographical Plan (scale 1:600) of the Proposed Site showing all the dimensions of the Site and Contours of the Land at 5m interval showing Nalas, Drains, Wells, Trees, Roads, Electricity Lines etc.
	
	
	

	4
	Proposed Layout Plans (scale 1:600) (1 Tracing Cloth/Film + 5 White /Ammonia Prints) duly signed by Land Owner, Developer, Architect
	
	
	

	5
	Plan showing rainwater harvesting pits
(scale 1:100) (as per G.O Ms.No.350 M.A dt.9.6.2000)

	
	
	

	6
	Photographs (4) & Videography showing four sides of the site.

	
	
	

	7
	Mortgage Plan (scale 1:100) 

	
	
	

	8
	Extract of Master Plan / ZDP  

	
	
	

	9
	Previous Development Permission Plan copy if issued previously.
	
	
	

	10
	Revenue Sketch issued by Revenue authority, if the site is part of S. Nos.
	
	
	

	NOCs

	1
	NOC from the Revenue Department under the Andhra Pradesh Agricultural Land (Conversion for Non-Agricultural Purpose) Act, 2006 
	
	
	

	2
	NOC from Revenue Department in case of lands abut Water bodies, Water courses & nalas with sketch plan with measurements. (wherever required)
	
	
	

	3
	NOC from Irrigation Department in case of lands abut water bodies, Water courses & nalas with sketch plan with measurements.(wherever required)
	
	
	

	4
	NOC from Railways (wherever required)

	
	
	

	5
	NOC from State Environmental impact Assessment Authority (wherever required)
	
	
	

	6
	NOC from Defence Authority (wherever required)

	
	
	

	7
	NOC from Oil / Gas Authority (wherever required)
	
	
	

	8
	NOC from the Competent Revenue Authority in case the land is declared as surplus


	
	
	

	9
	NOC from the District Collector wherever it is a Government Land allotted



	
	
	

	UNDERTAKINGS

	1
	Declaration-Cum-Undertaking on Rs.100/- Non Judicial Stamp Paper from the Owner, Licensed Architect  & Document Auditor 


	
	
	




	XII
	C E R T I F I C A T E   BY LAND OWNER & DEVELOPER

	I hereby certify that the information furnished in the application is true to the best of my knowledge. It is to further state that for the purpose of obtaining clearance under green channel, I have engaged the services of Sri.___________________________Empanelled Document Auditor and Sri.___________________________Empanelled Architect.
 They have after due diligence, certified correctness of information and the same are enclosed and form part of this application. In this regard if any information is suppressed (or) misrepresented I am aware that I am liable for action. 
I undertake that I will not change the Licensed Architect till the project is completed and if at all to change it will be done with mutual agreement and only on appointing another Licensed Architect who has been empanelled by HMDA and the change will be effected only after submission of the relevant agreements to HMDA and only after receipt of consent from HMDA. 

	1
	Name of the
Land  Owner

	

	
	Address 

	

	
	Phone:
	

	
	Signature of the 
Land Owner
	

	2
	Name of the Developer
	

	
	Address 

	

	
	License No. issued by HMDA:
	

	
	Phone:
	

	
	Signature of the 
Developer
	





